|  |  |  |  |
| --- | --- | --- | --- |
| **Campground ADA Checklist** | | | |
| Name of Campground: | | | |
| **Yes/No/NA Measurements/Comments** | | | |
| **RV Camping Spaces** |  |  | |
| Total number of RV camping spaces? |  |  | |
| How many camping areas are at least 20 feet wide? |  |  | |  | | |
| How many camping areas are at least 16 feet wide? |  |  | |
| Is the slope of the parking area 1:50 (2%) in any direction? |  |  | |
| \*\*However, where needed for proper drainage, an exception permits the slope to be up to 1:33 (3 percent) in any direction |  |  | |
| Is the running slope of a parking spur driveway up to 1:12 (8.33 percent) for 50 feet (15 meters)? |  |  | |
| \*\*An exception for areas of steeper terrain permits the running slope to be up to 1:10 (10 percent) for 30 feet (9 meters). |  |  | |
| Is the surface of each campsite firm and stable? |  |  | |
|  | **Compliant Site Number** | **Non-Compliant Site Number** | |
| **Walk in Camping Spaces**  **(see picture reference page attached)** |  |  | |
| Total number of walk in camping spaces? |  |  | |
| Is there a minimum 48-inch of clear floor or ground space around the tent platform area? |  |  | |
| Does the slope of the tent pad or platform exceed 1:50 (2 percent) in any direction? |  |  | |
| \*\*An exception permits the slope to be up to 1:33 (3 percent) maximum where needed for proper drainage. |  |  | |
| Is the surface of each pad or platform firm and stable? |  |  | |
|  | **Compliant Site Number** | **Non-Compliant Site Number** | |
| **Fire Ring, Fireplaces, Wood Stove**  **(see picture reference page attached)** |  |  | |
| Total number if fire rings, fireplaces and wood stoves? |  |  | |
| Is the fire-building surface within a fire ring a minimum of 9 inches above the floor or ground surface? |  |  | |
| Is there a clear floor or ground space at least 48 inches out from the ring or stove and at least 48 inches wide? |  |  | |
| Does the slope of the clear floor or ground space around the fire ring, fireplace or wood stove exceed 1:50 (2%) in any direction? |  |  | |
|  | **Compliant Site Number** | **Non-Compliant Site Number** | |
| **Water Hydrants**  **(water faucets and hand pumps)** |  |  | |
| Total number of water hydrants? |  |  | |
| Are hydrants located between 28 inches and 36 inches above the ground or floor surface? |  |  | |
| Is there a clear space of at least 60 inches by 60 inches? |  |  | |
| If there is a hand pump, does the force required to operate it greater than 5 pounds? |  |  | |
|  | **Compliant Site Number** | **Non-Compliant Site Number** | |
| **Utility Sinks**  **(see picture reference page attached)** |  |  | |
| Total number of utility sinks? |  |  | |
| Is there a clear floor or ground space of at least 30 inches by 48 inches, oriented for either a forward or side approach? |  |  | |
| Does the slope of the clear floor or ground space around the utility sink exceed 1:50 (2%) in any direction? |  |  | |
| Is the height of the counter or rim surrounding the sink more than 34 inches above the ground or floor space? |  |  | |
| Is the bottom of the bowl at least 15 inches above the ground or floor space? |  |  | |
| If hot water is provided, are the pipes wrapped or shielded to prevent someone from accidentally touching the hot pipes? |  |  | |
|  | **Compliant Site Number** | **Non-Compliant Site Number** |
| **Picnic Units Per Site**  **(see picture reference page attached)** |  |  |
| Does each site have at least one picnic table? |  |  |
| For tables up to 9 feet long, one space for wheelchair seating must be provided. Is this compliant? |  |  |  | |  |
| For tables between 10 feet and 18 feet long, two spaces for wheelchair seating must be provided. Is this compliant? |  |  |  | |  |
| Is the knee space for wheelchair seating at least 30 inches wide, 19 inches deep, and 27 inches high, as measured from ground to floor to the bottom of the tabletop? |  |  |
| Does the toe clearance measure at least 9 inches above the ground or floor and extend at least an additional 5 inches beyond the knee clearance? |  |  |
| Is there clear floor of ground space that is 30 inches by 48 inches provided at each wheelchair seating space and positioned to accommodate a forward approach to the table? |  |  |
| In addition the clear floor or ground space for wheelchair seating space, is there 48 inches of clear floor or ground space around the usable portions of the table? |  |  |
| Does the slope of the clear floor or ground space exceed 1:50 (2%) in any direction? |  |  |

|  |  |  |
| --- | --- | --- |
|  | **Yes/No/NA** | **Measurements/Comments** |
| **Benches**  **(see picture reference page attached)** |  |  |
| Total number of benches? |  |  |
| Is the font edge of the beach seat between 17 and 19 inches above the ground of floor space? |  |  |
| Do at least half of the benches have back support that runs the full length of the bench? |  |  |
| Of the benches with back support, do at least half of those have an armrest provided? |  |  |
| Is there a clear floor or ground space that is 30 inches 48 inches provided that is adjacent to one end of the bench? |  |  |
| Does the slope of the clear floor or ground space exceed 1:33 (3%) in any direction? |  |  |
| Is the surface under and around the bench firm and stable? |  |  |
|  |  |  |
| **Trash, Recycling, and Other**  **Essential Containers**  **(see picture reference page attached)** |  |  |
| Total number of containers? |  |  |
| Is there a clear floor or ground space of 30 inches by 48 inches provided to allow a forward or side approach? |  |  |
| Does the slope of the clear space exceed 1:50 (2%) in any direction? |  |  |
|  |  |  |
| **Cooking Surfaces, Grills, and Pedestal Grills**  **(see picture reference page attached)** |  |  |
| Total number of cooking surfaces, grills, and pedestal grills? |  |  |
| Is the height of the cooking surface 15 inches to 34 inches above the ground or floor surface? |  |  |
| Is there clear floor or ground space that is at least 48 inches deep and 48 inches wide, as measured from the cooking surface. |  |  |
| \*\*If a pedestal grill can rotate 360 degrees and all positions along that rotation are usable, the 48 inch clear space must completely surround the grill. |  |  |
| Does the slope of the clear space exceed 1:50 (2%) in any direction? |  |  |

Name of person who completed assessment: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Date: \_\_\_\_\_\_\_\_\_\_\_\_